Release Notes
-------------

Versions:
----------
4GIrisVDM:	3.2.0

Device SDK (AD100): 5.0.0

Device FirmWare Ver: 2.03

Release folder (Release_4G Iris VDM_ver3.2.0_13032013) consists of the following.

1. 4GIrisVDMInstaller.msi
2. 4GIrisVDMReleaseNotes_3.2.0.txt
3. 4G Iris VDM Installation Guide v2.0.pdf

Release Updates:
---------------
1. Updated the ISO header Format version from 020 to 010


FirmWare Update:
----------------
1. You check the current Firmware version on the Device LCD while it get Connected to Power or Click on the first button below the LED Screen on the device.
2. To Update the firmware, please go the C:\Program Files\4G Identity Solutions\4G Iris VDM\Utilities\Frimware and double click the Ad100Firmware V2_03.exe. Find More details at 4G Iris VDM Installation Guide v2.0.pdf.
3. Make sure device should not be disconnected while running the firmware update.


Install Instructions:
--------------------
1.Install by double clicking on 4GIrisVDMInstaller.msi
2.System restart may require after installation.
3.For more details of installation see the 4G Iris VDM Installation Guide ve 2.0

For Support Contact:
Ravikiran Gantasala
ravikiran.gantasala@4gid.com
Mobile: +91-9177787877
